**Model: Q2AM-CAM-4G-2.0MP**

**2.0 MP1080P 4G IP Camera**



**Camera Features:**

* 1/2.9"2.0 Mega Pixels Sony IMX323 CMOS sensor
* HD resolution 1920 x 1080P
* Motion detection, email alert, FTP upload
* Built-in IR Cut,No Color Cast.
* P2P, PNP: Plug&play, Support QR code scanning to view on Iphone and andriod Mobiles
* Support SIM Card,3G/4G.
* TF Card:Max to 128GB
* Water-proofhousing, IP66
* 2pcs IR Leds, IR distance 20-60 meters
* 2.7-13.5 mm Motorized lens
* Power Consumption: Day <2W,Night:<6W
* P2P APP:CamHi
* PC Software: P2P Client
* Audio:Two Ways.

**Technical Specifications:**

|  |  |
| --- | --- |
| **Model** | **Q2A-CAM-4G-2.0MP** |
| **Camera** |
| Image Sensor | 1/2.9"2.0 Mega pixels Sony IMX323CMOS |
| Chipset | Hi3516CV200+ IMX323 |
| Effective Pixels | 1920(H)×1080 (V) |
| Video Resolution  | 1080P@25/30fps  |
| Electronic Shutter | AUTO, 1/25 -1/50,000s, FLK, 1-30x |
| Min. Illumination  | 0.005Lux@F1.2(AGC ON), 0Lux IR on |
| Video  | 2 ways audio |
| Day/Night  | Auto/Color/(B/W)/EXT |
| Lens | 2.7-13.5mm Motorized Lens |
| USIM Card | 3G 4G Micro SIM Card |
| TF Card | Up to 128GB |
| IR Led | 2pcs IR Leds |
| IR Distance | 20-60M |
| Power Supply | 12 VDC ± 10% |
| Power Consumption | Day<1W, Night<3W |
| Operating Temp. | -20℃-(+60)℃, 10%-90%RH |